Addresses

|  |  |
| --- | --- |
| Discrete coils | 000001 – 065535 |
| Discrete inputs (contacts) | 100001 – 165535 |
| Input registers | 300001 – 365535 |
| Holding registers | 400001 – 465535 |

If other than default slave address is used it should be prefixed. For example 100:000001, where 100 is the slave address.